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	SYSTEM : DESIGNER TEXTURE FINISH FOR EXTERIORS

	Concrete and Masonry Surface – Exterior



System Description

Primary Coat: 1 coat Weathercoat AR Primer
A premium quality acrylic co-polymer based primer with good alkali resisting properties designed to provide a sound base for texture coating from the Berger range.

Volume Solids: 40% ± 2%

Top Coat: 2 coats of Select Rustic Décor
Select Rustic Decor is a Synthetic Render-cum-finish which can be applied straight to most fairface surfaces such as concrete, plaster, brickwork-both exterior and interior. Rustic Decor is a ready mixed coating composed of durable polymer resins, and, incorporating Different size & graded marble granules. With its unique engraved finish, Select Rustic Decor is truly a decorative plaster and a superb finish-both in one. Rustic Decor incorporates fungicides and algaecides which give good microbial resistance. Select Rustic Decor has Good Ultra Violet (UV) resistance & adhesion on various surfaces. Select Rustic Decor has a ‘Breathable Film’ that breathes out trapped moisture both from the paint surface as well as the substrate.

Volume Solids: 70% ± 2%

Recommended Areas of Application
Area of Use: Exterior & Interior
Substrate: Concrete, Plaster, Masonry, Brickwork, Block work, Timber.
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