Outdoor 60 cm single sided NTP Synchronised Analogue Slave Clock (model Profil 960 E or equivalent) 

The slave analogue outdoor clock shall have a 60 cm dial diameter with black hour and minute hands.  
The clock shall have an ABS casing with swivel opening. The crystal shall be shatterproof and non reflective. The viewing distance shall be 60 metres. The clock shall be backlit by white LEDs.
The index protection shall be at least IP53 for outdoor use.

Choice of 
Time display: hour, minute or hour, minute and second.
Dial marking: Arabic figures or notches or DIN marking.
Casing colour: white.

Slave clock operation with NTP network time signal.
The power shall be supplied by the 230V AC mains.
The slave clock shall have a RJ 45 connector. 
The clock shall have plug and play features with no settings required. Upon reception of the time signal, the clock shall automatically and immediately adjust itself to the correct time. In case of loss of the time signal the clock shall operate on its own time base until signal recovery. 
The time information shall be continuously saved.

  

Outdoor 60 cm double sided NTP Synchronised Analogue Slave Clock (model Profil 960 E Double sided or equivalent)

The secondary analogue outdoor clock shall have a 60 cm dial diameter with black hour and minute hands.  
The clock shall have a double sided casing with bracket, each side with swivel opening. The crystal shall be shatterproof and non reflective. The viewing distance shall be 60 metres. The clock shall be backlit by white LEDs. 
The index protection shall be at least IP53 for outdoor use.

Choice of 
Time display: hour, minute or hour, minute and second.
Dial marking: Arabic figures or notches or DIN marking.
Casing colour: white.

Slave clock operation with NTP network time signal.
The power shall be supplied by the 230V AC mains.
The slave clock shall have a RJ 45 connector. 
The clock shall have plug and play features with no settings required. Upon reception of the time signal, the clock shall automatically and immediately adjust itself to the correct time. In case of loss of the time signal the clock shall operate on its own time base until signal recovery. 
The time information shall be continuously saved